ReadMe

Thank you for downloading the bve Joetsu Line (Minakami `->` Echigo-Nakazato).

[Image] 1739M, 07.6.16 [右]9079, 05.2.16 [左]EF16 28, 07.6.16

1. First

This route works with BVE 2.6 and BVE 4.2.
`Route :`JR Joetsu Line
`` Minakami Sta. `->` Echigo-Nakazato Sta.
`Version:`beta 0.20 （2008-12-24 updated）
`producer:`k_40s2
`Web Site:`http://gri.s60.xrea.com/
`E-mail :` k_40s2@ybb.ne.jp

2. Installation
| If BVE folder and mackoy folder don't locate same rank or 40's-2 is omitted, it don't find train file or don't read timetable image for BVE4 dates. In this case, rewrite pass of train file or timetable image in route file.

3. Train

LOCAL 1729M
Minakami Sta. 13:44 `->` Echigo-Nakazato Sta. 14:11
Series 115, 3 cars (BVE2)
(115-1000_kame, Get from "Ellis and Tommy BVE Page")
Series 113, 6 cars (BVE4, substitute)
(113_6)
Exp. FREIGHT 9079
Minakami Sta. 13:10 `->` Echigo-Nakazato Sta. 13:41
Class EF16 2cars FC600t (substitute)
(EF16, Get from "Wai's room" : http://waisroom.sakura.ne.jp/)

4.Driving
| (1) Sign signal and limit speed

Limit sppeed of this route is 110km/h, but the limitation of 1739M is 100km/h and 9079 is 75km/h. Protection system is ATS-Sn.
Limit speed of sign signal is as follows.

Stop | Limitation is 25km/h | Limitation is 45km/h | Limitation is 65km/h | No speed limitation

| (2)Marker

A. Relate fot diriving train

Speed limit post | Speed limit post for switch For left turn in this case | Resume speed limit post Not putted in the length less than 100m or for switch

Signal call point marker | Train stop indicator If train overruns on this side, it can go back | Train stop marker

S marker Limiting speed from here in extraoridinary weather | O marker Limiting speed to here in extraoridinary weather | Unknown All 10 cars go out from speed limited area

Section gap marker Do not stop ahead hear because prevent wire break |  |

B. Others

Distance post | Successive post | Curve post

Grade post The number means grade per kilometer | Station approach marker | Switch over speed alarm marker

Crossing number marker | Starting signal marker For conductor No relation fot diriving train | Shunting indicator No relation fot diriving train

Car stop indicator No relation fot diriving train | Caution marker for snowplow No relation fot diriving train |

| (3)Speed limit

At the curve
･Common EMU (Ex. Series 115) : Speed in curve +5km/h (75km/h in right image)
･High-performance EMU (Ex. Series 485) : Speed in curve +10km/h (80km/h in right image)
･Conventional train : Speed in curve +0km/h (70km/h in right image)
On the decline
･`Doai `->` Tsuchitaru` : -5km/h from max speed of car
･`Tsuchitaru `->` Echigo-Nakazato` : -15km/h from max speed of car
Speed limit on the decline at exit of Shin-Shimizu tunnel is -15km/h from max speed of car.
((cf. Max speed of car))
Series 115 : 100km/h, Series 485 : 120km/h, EF16 : 75km/h, Koki50000 : 95km/h

Copyright(C) 2003-2008 k_40s2（きまぐれforties2号）