EM A1 
3D Cab Animated
Rel. 1.00 23/10/2009

Electric Passenger Train 
on FEVF and FGC routes 
by S.Usai and R.Benini
for OpenBve only

Characteristics:
Construction: T.I.B.B. and Carminati Toselli.  
Year construction: 1929 
Gauge: 1000 mm 
Wheel pattern: Bo-Bo
Diameter wheels: 930 mm 
Length: 15480 mm 
Width: 2600 mm 
Tension to the line of contact: 2400 vcc 
Number motor: 4 type GDTM08 4 poles etc. series 
Nominal motor tension: 2400v/2 
Max. Power: 87 kw to 730 rpm 
Max. Speed: 60 km/h 
Weight to full load: 36800 kg 
Starting: reostatic

The original EM A1 for BVE2 by Sergio Usai 
http://fgc.altervista.org/bve.htm
has been modified and suited 
with the consent of the author
by Roberto Benini 
http://fgc.altervista.org/bve.htm

Caratteristiche:
Elettromotrice a carrelli 
Costruzione: T.I.B.B. e Carminati Toselli. 
Anno costruzione: 1929
Scartamento: 1000 mm
Rodiggio: Bo - Bo
Diametro ruote: 930 mm
Lunghezza: 15480 mm
Larghezza: 2600 mm
Tensione alla linea di contatto: 2400 vcc
Numero motori: 4 tipo GDTM08 4 poli ecc. serie
Tensione nominale motore: 2400v/2
Potenza oraria: 87 kw a 730 giri
Velocità massima: 60 km/h
Peso a pieno carico: 36800 kg
Avviamento: reostatico

La versione originale della EM A1 BVE2 di Sergio Usai
http://fgc.altervista.org/bve.htm
è stata modificata e adattata
con il consenso dell'autore
da Roberto Benini
http://fgc.altervista.org/bve.htm

