ENGLISH ELECTRIC TYPE 4, LATER BR CLASS 50 DIESEL-ELECTRIC LOCO.

Consist = 10 mk2 air-cons.

Engine = EE 16CSVTmk2
Continuous rating 2700 hp
Continuous tractive effort 33000 lb at 23.5 mph
Weight 117 ton
Wheel arrangement Co-Co
Length over buffers 68ft 9in
Driving wheel diameter 3ft 7in
Maximum permitted speed 100 mph
Overload current 2500amps

