=======================================
LT 1995 Stock openBVE v 10.04.09
---------------------------------------
Steve Green Miles Codrington & Dan Lewis
=======================================

(c) Miles Codrington / Dan Lewis / Steve Green 2005 - 2009.

Cab graphics by Miles Codrington and Steve Green
Sound arrangement, and physics by and (c) Dan Lewis & Steve Green.
Sounds (c) Dan Lewis & Steve Green except for Motor0.wav thanks to John Owen. Whistle and run sounds sampled from the video125 Northern Line cab ride with grateful permission. 
Reference photos thanks to Richard Randall (http://www.piccadilly-line.org.uk) Chris Cobley
Passing bridge sound mixed with one created originally by Anthony Bowden.
Animated wiper with thanks to Martin Finken
External model by Steve Green with thanks to Anthony Bowden for the pointers for the animation code, and Neil and Tom for testing.

High Resolution OpenBVE Version uses the OS_ATS plugin by Oskari Saarekas
-------------------------------------------------------

This train features LU Tripcocks, Rail Gap current loss & Left / Right door release.

If you run through a red signal you will be braked to a stop, and will get a message on the console. You must wait until that signal has cleared, then press SPACE to reset the tripcock system before preceding.

You may pass a red signal with authority by pressing HOME prior to the signal. This will allow you to pass the next signal at danger.

As your train passes gaps in the electric rail the current will be momentarily lost.

KEY PRESSES:
------------

HOME   = will give temporary tripcock isolation
SPACE  = will reset a brake application caused by a tripcock
PageUp = will turn on the wiper (and toggle between full wipe and intermitant)
PageDn = will turn off the wiper
+ key  = will make an door closing announcement

F5 - open/close left doors
F6 - open/close right doors

Top row number keys +

4      = Toggle destination indicator 
5      = Toggle HEADLAMPS / TAILLAMPS
6      = Toggle Saloon lights on/off
8      = cut out left side end doors for short platforms (press before giving door release and press again after door closure)
0      = cut out right side end doors for short platforms (press before giving door release and press again after door closure)



**If you jump stations the tripcock may apply the brakes if you jump past red signals. To reset, place the controller to OFF and the reverser to NEUTRAL. Press SPACE. The brake should then release, and you can carry on as normal**

Please seek permission before using any
material from this train in your own add-ons.

Train Sim Central 

- www.trainsimcentral.co.uk -


