[Object]
States = 92BOpenBVE.csv

;RIGHT HAND SIDE DOORS

[Object]
Position = 0.01, 0, -3.74
States = doorright.csv
TranslateZFunction = -rightdoors[0]

[Object]
Position = 0.01, 0, -2.46
States = doorright2.csv
TranslateZFunction = rightdoors[0]

[Object]
Position = 0.01, 0, 1.08
States = doorright.csv
TranslateZFunction = -rightdoors[0]

[Object]
Position = 0.01, 0, 2.28
States = doorright2.csv
TranslateZFunction = rightdoors[0]

[Object]
Position = 0.01, 0, 5.99
States = doorright.csv
TranslateZFunction = -rightdoors[0]

[Object]
Position = 0.01, 0, -7.47
States = doorright2.csv
TranslateZFunction = rightdoors[0]


;LEFT HAND SIDE DOORS

[Object]
Position = -0.01, 0, -3.74
States = doorleft.csv
TranslateZFunction = -leftdoors[0]

[Object]
Position = -0.01, 0, -2.46
States = doorleft2.csv
TranslateZFunction = leftdoors[0]

[Object]
Position = -0.01, 0, 1.08
States = doorleft.csv
TranslateZFunction = -leftdoors[0]

[Object]
Position = -0.01, 0, 2.28
States = doorleft2.csv
TranslateZFunction = leftdoors[0]

[Object]
Position = -0.01, 0, 5.99
States = doorleft.csv
TranslateZFunction = -leftdoors[0]

[Object]
Position = -0.01, 0, -7.47
States = doorleft2.csv
TranslateZFunction = leftdoors[0]

;axels

[Object]
States = axel.csv
Position = 0, 0.16, 5.4
RotateXFunction = value + delta * speedometer / 0.15

[Object]
States = axel.csv
Position = 0, 0.16, 3.35
RotateXFunction = value + delta * speedometer / 0.15

[Object]
States = axel.csv
Position = 0, 0.16, -3.6
RotateXFunction = value + delta * speedometer / 0.15

[Object]
States = axel.csv
Position = 0, 0.16, -5.65
RotateXFunction = value + delta * speedometer / 0.15