Class 47 Diesel Loco

Max Speed: 95-100 mph
Built by Brush/BR Crewe
Introduced: 1963-67
Engine: Sulzer 12-cyl
Engine BHP: 2750 @ 750rpm (1,920kW)
Transmission: Electric
Max. Tract. Effort: 55,000-60,000 lb/f
Cont. Tract. Effort: 33,000lb/f @ 26mph
Power at Rail: 2080hp (1550kW)

Weight: 114-125 ton
R.A.: 6 or 7
Brake force: 60 ton
-------------------
Consist: 1 + 8 Mk 2 coaches
-------------------

trainsimcentral.co.uk