[Object]
States = 1311.csv
Position = 0,0,-12.95

;Wheels;
[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = 0.744,0.655,-10.95

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = -0.744,0.655,-10.95

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = 0.744,0.655,-9.55

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = -0.744,0.655,-9.55


[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = 0.744,0.655,6.05

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = -0.744,0.655,6.05

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = 0.744,0.655,7.55

[Object]
States = wheels.csv
RotateXFunction = value + delta * speedometer / 0.505
Position = -0.744,0.655,7.55

;Interior Walls;
[Object]
States = intwall3.csv
Position = 0.008,0,-11.75

[Object]
States = intwall.csv
Position = 0.008,0,-6.38

[Object]
States = intwall.csv
Position = 0.008,0,-1.02


[Object]
States = intwall.csv
Position = 0.008,0,4.35

[Object]
States = intwall4.csv
Position = 0.008,0,9.72

;Door 1;

[Object]
States = drsl_left.csv
Position = 0.008,0,-9.06
TranslateZFunction = -max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = drsl_right.csv
Position = 0.008,0,-9.06
TranslateZFunction = max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = doorbottom_left.csv
Position = 0,0,-9.06

[Object]
States = drsr_left.csv
Position = -0.008,0,-9.06
TranslateZFunction = -max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = drsr_right.csv
Position = -0.008,0,-9.06
TranslateZFunction = max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = doorbottom_right.csv
Position = 0,0,-9.06

;Door 2;

[Object]
States = drsl_left.csv
Position = 0.008,0,-3.73
TranslateZFunction = -max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = drsl_right.csv
Position = 0.008,0,-3.73
TranslateZFunction = max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = doorbottom_left.csv
Position = 0,0,-3.73

[Object]
States = drsr_left.csv
Position = -0.008,0,-3.73
TranslateZFunction = -max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = drsr_right.csv
Position = -0.008,0,-3.73
TranslateZFunction = max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = doorbottom_right.csv
Position = 0,0,-3.73

;Door 3;

[Object]
States = drsl_left.csv
Position = 0.008,0,1.66
TranslateZFunction = -max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = drsl_right.csv
Position = 0.008,0,1.66
TranslateZFunction = max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = doorbottom_left.csv
Position = 0,0,1.66

[Object]
States = drsr_left.csv
Position = -0.008,0,1.66
TranslateZFunction = -max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = drsr_right.csv
Position = -0.008,0,1.66
TranslateZFunction = max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = doorbottom_right.csv
Position = 0,0,1.66

;Door 4;

[Object]
States = drsl_left.csv
Position = 0.008,0,7.03
TranslateZFunction = -max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = drsl_right.csv
Position = 0.008,0,7.03
TranslateZFunction = max[(power[min[leftdoors[0]*1.2,1],2]+1-power[(1-max[(leftdoors[0]-0.5)*1.2,0]),3])/2,(power[min[leftdoors[0]*4,0.9],2])/4-leftdoorstarget]*0.87

[Object]
States = doorbottom_left.csv
Position = 0,0,7.03

[Object]
States = drsr_left.csv
Position = -0.008,0,7.03
TranslateZFunction = -max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87

[Object]
States = drsr_right.csv
Position = -0.008,0,7.03
TranslateZFunction = max[(power[min[rightdoors[0]*1.2,1],2]+1-power[(1-max[(rightdoors[0]-0.5)*1.2,0]),3])/2,(power[min[rightdoors[0]*4,0.9],2])/4-rightdoorstarget]*0.87
[Object]
States = doorbottom_right.csv
Position = 0,0,7.03

;Seats;
[Object]
States = blue/short_1.csv
Position = 0,0.65,8.31

[Object]
States = blue/long.csv
Position = 0,0.65,3

[Object]
States = blue/long.csv
Position = 0,0.65,-2.4

[Object]
States = blue/long.csv
Position = 0,0.65,-7.8

[Object]
States = blue/short_3.csv
Position = 0,0.65,-12.76

[Object]
States = blue/short_2.csv
Position = 0,0.65,8.31

[Object]
States = blue/long_left.csv
Position = 0,0.65,3

[Object]
States = blue/long_left.csv
Position = 0,0.65,-2.4

[Object]
States = blue/long_left.csv
Position = 0,0.65,-7.8

[Object]
States = blue/short_4.csv
Position = 0,0.65,-12.76