OPENBVE
#CAR
+0078.0                  ;Powr_Cars MTON
+000001                  ;Powr_Cars NMBR,Always Use 1 For Correct Cplr Action
+0050.0                  ;Trlr_Cars MTON
+000000                  ;Trlr_Cars NMBR=Trlr_Cars+EndOfTrainDvic+Powr_Cars-1
+0014.4                  ;Avrg_Lgth METR
+000001                  ;Trlr_Cars@FRNT,Powr_Cars@FRNT=0or1
#CAB
+000800                  ;View_DimX MMTR
+002915                  ;View_DimY MMTR
-003275                  ;View_DimZ MMTR
#DEVICE
+000000                  ;Sfty_Stop DSBL 
+000000                  ;Sfty_Ctrl DSBL
+000000                  ;Sfty_Vigl DSBL
+000001                  ;Thrt_Auto ENBL
+000000                  ;Brak_Hold DSBL
-000001                  ;Slip_Ctrl DSBL
#HANDLE
+000000                  ;Brak+Thrt ENBL
+000008                  ;Thrt_Nmbr 0to8
+000008                  ;Brak_Nmbr 0to8
+000000                  ;Thrt_Rset 0to8,Dflt=0
#BRAKE
+000000                  ;Syst_Type:RLES~PNEU_1toX~EMRG=0,RLES~ELEC_1toX~EMRG=1,RLES~LAPD~SRVC~EMRG=2
+000000                  ;Dyna_Type:PNEU+DYNA=0,DYNA>KPHR=1,DYNA@FRST=2
+009999                  ;Dyna_Minm KPHR,Dsbl=9999
#PRESSURE
+000441                  ;Cyli_Srvc,BRIT=00480kpag=00070psig,AARX=00441kpag=00064psig=Pipe_Maxm*5/7
+000531                  ;Cyli_Emrg,BRIT=00480kpag=00070psig,AARX=00531kpag=00077psig=Pipe_Maxm*6/7
+000855                  ;Rsvr_Minm,BRIT=00690kpag=00100psig,AARX=00855kpag=00124psig
+000910                  ;Rsvr_Maxm,BRIT=00780kpag=00113psig,AARX=00910kpag=00132psig
+000620                  ;Pipe_Maxm,BRIT=00490kpag=00071psig,AARX=00620kpag=00090psig
#DELAY
+003.00                  ;Thrt_Incr SECS
+002.00                  ;Thrt_Decr SECS
+001.00                  ;Brak_Aply SECS
+001.00                  ;Brak_Rles SECS
+001.00                  ;Emrg_Aply SECS
+001.00                  ;Emrg_Rles SECS
#MOVE
+008000                  ;Thrt_Incr VIBS
+004000                  ;Thrt_Decr VIBS
+002000                  ;Brak_Emrg VIBS
+001000                  ;Brak_Srvc VIBS
+000500                  ;Brak_Dyna VIBS
+000250                  ;Brak_Rles VIBS
#DECELERATION
+001.80                  ;Dcel_Emrg M/S2
+000.25                  ;Dcel_Fric M/S2
#ACCELERATION
+000.25,+000.50,000,015  ;Acel_Thr1 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.30,+000.60,005,030  ;Acel_Thr2 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.35,+000.70,010,045  ;Acel_Thr3 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.40,+000.80,015,060  ;Acel_Thr4 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.45,+000.90,020,075  ;Acel_Thr5 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.50,+001.00,025,090  ;Acel_Thr6 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.55,+001.10,030,105  ;Acel_Thr7 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
+000.60,+001.20,035,120  ;Acel_Thr8 M/S2 Minm,M/S2 Maxm,KPHR Minm,KPHR Maxm
